client
auth-user-pass
proto udp
dev tun
# CHANGE THIS TO MATCH YOUR SETUP PUBLIC IP ADDRESS
remote 66.66.66.66 1194
cipher AES-256-CBC
user nobody
group nogroup
verb 2
mute 20
keepalive 10 120
comp-lzo
persist-key
persist-tun
float
resolv-retry infinite
nobind
